Chapter 4. Prepaid

Prev. | Chapter 4. Prepaid

## Chapter 4. Prepaid

4.1. List of meters
4.2. The state of prepaid
4.3. The settings of prepaid и

### 4.1. List of meters

Immediately after the discovery of this page will be displayed: serial number, model and memo. Other cells will display "?" (no data available).
There are two ways to check your current balance:
1) select the required meters from the list and click Read Selected;
2) click Read All, accordingly, the software will try to get data from all meters;
It takes time to receive data.
After the exchange with the meter, the status column should display the result of the query, if OK) - the exchange has ended successfully? - there was no exchange, something else - an exchange error occurred. If the exchange has ended successfully, then with a single click, the left mouse button on the meter will show the detailed state of the meter:
1) The state of prepaid;
2) The settings of prepaid и;
3) The amount of energy consumed;
4) The temperature of the meter.
If, however, the click will be double, then prepaid preference settings for the selected meter will be displayed, if any.

### 4.2. The state of prepaid

After the exchang with the meter, you can view the detailed state of prepaid in the meter. To do this, go to the Prepaid tab, click on the desired meter in the table. Then, on the Prepaid tab, the fields: Balance, Value of the last refill, Last charge date, Relay status (picture), Table of consumed energy on prepaid will be filled with corresponding values.
To recharge is necessary:
1) select the required meter in the table;
2) click Charge;
3) enter the amount of replenishment from 1 to 5'000'000 monetary units;
4) check the details of the replenishment, if everything so after the approval of the software will try to contact the meter and record in it the amount of replenishment;
The possibility of cancellation of the amount of the account in the meter is provided; for this purpose, when replenishing, it is necessary to enter the required amount with the sign "-", the amount of write-off can not be less than -100'00 monetary units;
Before the account is replenished, the meter is checked after replenishment, if this amount is more than 15'000'000 monetary units or less than -100'000 monetary units - the operation will be canceled;

### 4.3. The settings of prepaid

Once the meter is successfully exchanged, you can view the detailed prepaid status in the meter. To do this, you must double-click the left mouse button on the desired meter from the list. This will activate the Configuration tab where the current prepaid settings for the meter will be displayed: the cost of consumed energy by tariffs, display parameters and relay switching off.
To write prepaid settings, you must:
1) select the required meter from the list;
2) select the required prepaid profile in the drop-down list, except for the first item (displays the settings for the current meter);
3) press Write, wait for the result of exchange with the meter;
To the right of the Write button, there is a drop down list of saved profiles for prepaid.
You can modify/add/remove them. To do this, select the desired profile and, depending on what you need, click Edit (Picture of the pencil) or Add (Picture Plus).

In the window that opens, you can specify the necessary options for the prepaid, such as:
1) the price for 1 kW / hour (the monetary unit does not matter, it is only for a better understanding that it is a money);
2) display parameters;
3) relay switching settings: power limit, switch off threshold, do not switch off, do not switch off after switching off by Sat, Sun;
To save the changed settings, click OK.

Prev. | Chapter 4. Prepaid